BusinessPhone Communication Platform 5.1
Commands > Commands 1000...1999

## 1936
Prefix calling number for E.164 number plan with international type of number

Specifies prefix digits for international calls. The prefix is included as predigits to the received calling/connected party number from the ISDN network.

##### The complete number is used for

- displaying on system phones
- caller list
- call logging of A-number

##### Valid values: 0-4 digits (0-9,*,#)

Revision: PD1 © Ericsson Enterprise 2003