BusinessPhone Communication Platform 5.1
Commands > Commands 3000...3999

## 3067
Control messages for others

In order to be able to restrict the number of extensions with access to certain facilities, such extensions are assigned A-category (ACOS) via command 0101 Facility COS.

This command is used to state for which A-category/categories) it is permitted to control (monitor, erase, etc.) the messages of others.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD4 © Ericsson Enterprise 2003