BusinessPhone Communication Platform 5.1
Commands > Commands 9000...9999

## 9138
Send expensive route warning tone 3

This command defines if the user shall be informed about an alternatively chosen PNR route (e.g. a public route) for the ongoing call setup.

In order to hear the Expensive Route Warning Tone, the command 0187 has to be set for the extensions.

Valid data

Valid values: YES / NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003