BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## A0 TRANSM

02h TRMCONREQ |  | Transmission connection request |
03h TRMCONSPK |  | Transmission speech connection |
04h TRMCONNOM |  | Transmission nominal (no speech) |
05h TRMCONADJ |  | Transmission adjusted (no speech) |
0Ah TRMREP |  | Transmission report |
0Bh TRMREP2 |  | Transmission report 2 connected channels |
12h TRMCON |  | Transmission connect |
13h TRMADJ |  | Transmission connect, adjusted levels |
14h TRMNOM |  | Transmission connect |
21h TRMACK |  | Transmission levels okay |
22h TRMNAK |  | Transmission levels not okay |
25h TRMWARNING |  | Warning in SX |

Revision: PD2 © Ericsson Enterprise 2003