BusinessPhone Communication Platform 5.1
Commands > Commands 0000...0999

## 0153
Direct carrier access?

The command defines whether or not the extension is permitted to select a specific carrier by dialling its access code. The call will then not be controlled by LCR functions, day-of-week and time-of-day analysis. LR will however eventually add account- and authority codes according to the carrier definitions.

Valid data: |  |
Yes |  | Allowed to select a carrier directly |
No (default) |  | Not allowed to select a carrier directly |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD6 © Ericsson Enterprise 2003