BusinessPhone Communication Platform 5.1
Dialogs

## Programmable Key Function Selection

You can edit a programmable key and select a key function. When a key is selected from the Programmable Keys dialog, the current configuration of the key is displayed.

Depending on the selected key function, only relevant input parameters can be changed in this dialog. When submitting parameter changes, these changes are applied to the Programmable Keys dialog. To save the changes, use the Programmable Keys dialog.

To access the dialog, click on the “Extensions...” menu in the Configuration directory tree and select “List extensions”. Now click on an extension’s link in the Directory Number column. The Extension Parameter dialog opens. On top of the dialog, you can see a navigation bar. Click on “Programmable Keys”. In the “Key resources” section, click on an extension button “...” on the right side of each extension.

Note

The displayed data depends on the extension type, the extension assignment, the system connection mode and on the system version. Additionally, the dialog may look different in offline and online mode.

The following commands and settings are available:

|  | Key number

- Enter the number of the respective key.

0301 |  | Key function

- Select a key function from the drop-down list.

0302 |  | Number/Id

- Enter the number or ID.

0303 |  | Ring alternative

- Select a ringing alternative from the drop-down list.

0304 |  | Priority

- Select a priority setting from the list.

#### Actions

Set |  | To apply the changed parameters in the programmable key dialog. |
Previous |  | To go to the previous key number. |
Next |  | To go to the next key number. |
Close |  | To close the dialog. |

See also facility descriptions:

- General (15534-ASB 150 02 Uen).
- Programmable And Fixed Keys (404/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2003