BusinessPhone Communication Platform 5.1
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 4F CONRELCTRL

00h CRCREGNEW |  | Release, start with new regtone |
01h CRCREGKEEP |  | Release, start with new regtone, keep proc |
02h CRCCBBOOK |  | Release, book for specified party |
03h CRCACDRERO |  | Release from ACD, reroute |
04h CRCLCRBUSY |  | No free trunk after Least cost routing anal |
05h CRCCALLPROG |  | Release with progress info from net |
06h CRCPICKUP |  | Pickup common bell extension not allowed |
07h CRCPICKUPNR |  | Pickup common bell extension not allowed, extension not in ringing state |
08h CRCDISA |  | Setup of transit call after successful DISA login |
09h CRCALTROUTE |  | Alternative routing because of a network specific reason |
0Ah CRCROP |  | 'Switch over' of an ongoing IP-call |
0Bh CRCRESTONE |  | Release connection by the called party requesting special tone |

Revision: PD2 © Ericsson Enterprise 2003