BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4308
No answer to sender (days)

This command states for how many full days (24-hour periods) a message may remain unanswered before the sender is notified that the message is still unanswered. Range of values 0-99.

Counting starts at midnight after the message has been sent. The sender is then notified at midnight after the programmed number of days. Value 0 means that the sender is notified already at midnight on the same day the message was sent.

Note

If the parameter value in command 4304 Time to keep message is identical with or lower than the value selected here, the message will be erased before the time elapses, i. e. the sender will never be notified that the message has not been answered.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003