BusinessPhone Communication Platform 5.1
Facility Description – General

## ASB 150 02 – Features

Description of features available with certain types of telephones

### Digital / IP / Cordless Phones

Digital / IP/ Cordless Phones Feature (Blatt 1 von 3) | Digital | IP |  | Cordless
DBC 210 | DBC 211 | DBC 212 | DBC 213 | DBC 213 + 2 DSS | DBC 213 + 4 DSS | DBC 214 | DBC 214 + 2 DSS | DBC 214 + 4 DSS | DBC 413 | Standard H.323 client | DT 290 | DT 4x0 | DT 570
Abbreviated no. dial. – common numbers | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Abbreviated no. dial. – individual numbers via key pad | 10 | 10 | 10 |  |  |  |  |  |  | X | X | 10 | 10 | 10
Abbreviated no. dial. – individual numbers via prog. key |  | 4 | 4 | 14 | 48 | 82 | 3 | 37 | 71 |  |  |  |  |
Account numbers | X | X | X | X | X | X | X | X | X | X | X | X | X | X
ACD agent-tel. |  | X | X | X | X | X |  |  |  |  |  |  |  |
ACD supervisor-tel. |  |  | * | X | X | X |  |  |  |  |  |  |  |
Alarm function | X | X | X | X | X | X | X | X | X |  |  |  |  |
Authority code | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Automatic callback | X | X | X | X | X | X |  |  |  | X | ** | X | X | X
Automatic Redial | X | X | X | X | X | X | X | X | X |  |  |  |  |
Automated Attendant | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Background music | X | X | X | X | X | X | X | X | X |  |  |  |  |
Bypass call diversion and follow me | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Call metering |  |  | * | X | X | X | * | * | * |  |  |  |  |
Call p. up - common | X | X | X | X | X | X | X | X | X |  |  |  |  |
Call p. up - ext. group | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Call p. up - individual | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Call waiting indic. | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Camp on | X | X | X | X | X | X | X | X | X |  |  | X | X | X
Clock and diary |  |  | X | X | X | X | X | X | X | *** | *** | X |  | X
Common bell | X | X | X | X | X | X | + | + | + | X | X | X | X | X
Conference | X | X | X | X | X | X | * | * | * | X | ** | X | X | X
Conn. state mess. | X | X | X | X | X | X | X | X | X |  |  | X | X | X
Conversation recording | X | X | X | X | X | X |  |  |  |  |  |  |  |
CT (Computer Telephony) | X | X | X | X | X | X | * | * | * | ## | ## | X | X | X
CTI-Groups | X | X | X | X | X | X | X | X | X |  |  | X | X | X
Dictaphone function | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
DISA | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Diversion direct | X | X | X | X | X | X | # | # | # | X | X | X | X | X
Diversion on busy | X | X | X | X | X | X |  |  |  | X | X | X | X | X
Div. on no reply | X | X | X | X | X | X | # | # | # | X | X | X | X | X
Doorph. (answering) | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Fault indication |  |  |  | X | X | X | X | X | X |  |  |  |  |
Follow me | X | X | X | X | X | X |  |  |  | X | X | X | X | X
Group hunting | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Hot line | X | X | X | X | X | X |  |  |  | X | X | X | X | X
Hotel guest room tel. | X | X | X |  |  |  |  |  |  | X | X | X | X | X
Hotel reception tel. |  |  |  | X | X | X | X | X | X |  |  |  |  |
Hotel service tel. |  |  | X | X | X | X |  |  |  |  |  |  |  |
Immediate answer |  | X | X | X | X | X | X | X | X |  |  |  |  |
Information | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Inquiry | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Intercom | * | X | X | X | X | X | X | X | X |  |  |  |  |
Intrusion | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
ISDN Caller List |  |  | X | X | X | X |  |  |  |  |  | X | X | X
ISDN Calling Line Id. |  |  | X | X | X | X | X | X | X | X | X | X | X | X
ISDN Connected Line Identification |  |  | X | X | X | X | X | X | X | X | ### | X |  | X
Key system function | X | X | X | X | X | X | X | X | X |  |  |  |  |
Last ext.numb.redial | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Least Cost Routing | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Loudspeaker paging | X | X | X | X | X | X | X | X | X |  |  |  |  |
Mailbox-sys. comm. | X | X | X | X | X | X | X | X | X | X | ** |  |  |
Mailbox-sys. indiv. | X | X | X | X | X | X |  |  |  | X | ** | X | X | X
Message-sys. voice | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Message-s. call me | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Message-sys. text |  |  |  | X | X | X | X | X | X |  |  |  |  |
Name selection | X | X | X | X | X | X | X | X | X |  |  |  |  |
Night service | * | X | X | X | X | X | X | X | X | * | * | * | * | *
Paging | X | X | X | X | X | X | X | X | X |  |  | X | X | X
Park.for com.access | X | X | X | X | X | X |  |  |  | X | ** | X | X | X
Parking individual | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Private trunk line | X | X | X | X | X | X | X | X | X |  |  |  |  |
Programmable and fixed keys | 3 | 4 | 4 | 14 | 48 | 82 | 3 | 37 | 71 |  |  |  |  |
Refer back | X | X | X | X | X | X | X | X | X | X | ** | X | X | X
Reminder service | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Saved ext. no. redial | X | X | X | X | X | X | X | X | X |  |  |  |  |
Secretary function | * | X | X | X | X | X | X | X | X |  |  |  |  |
Supervision | X | X | X | X | X | X | X | X | X |  |  |  |  |
Tandem - Slave | X | X | X | X | X | X |  |  |  | X | X | X | X | X
Tandem - Master | X | X | X | X | X | X |  |  |  | * | * | * | * | *
Telephone directory |  |  |  | X | X | X | X | X | X |  |  | * | * | *
Trunk line key | X | X | X | X | X | X | X | X | X |  |  |  |  |
Voice mail box, external | X | X | X | X | X | X | X | X | X |  |  | X | X | X

* |  | available with limitations

** |  | if instrument supports suffix dialing & hookflash

*** |  | only locally from instrument, no update from ASB 150 02

^ |  | available if you use the feature: "Abbreviated number dialling - common numbers"

+ |  | can not be programmed as Common bell, but only answer calls

# |  | corresponds to the feature "Offduty position"

## |  | supports only pots functionality

### |  | if supported by instrument

### Analogue telephones, mobile extension, old digital and cordless phones

Analogue & old digital and cordless phones Feature (Blatt 1 von 3) | Analogue | Mobile extension | Digital | Cordless
rotary | DTMF | DBC 751 | DBC 755 | DBC 753 | DBC 754 | DBC 199 | DBC 601 | DBC 631 | DBC 662 | DBC 663 | DBC 360 | DBC 368
Abbreviated no. dial.- common numbers | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Abbreviated no. dial.- individual numbers via key pad | ^ | 10 | 10 | 10 |  |  |  | 10 | 10 |  |  |  | 10 | 10
Abbreviated no. dial.- individual numbers via prog. key |  |  |  |  | 10 | 30 | 20 |  |  | 10 | 30 | 20 |  |
Account numbers |  | X | X | X | X | X | X | X | X | X | X | X | X | X
ACD agent-tel. |  |  |  |  | X | X |  |  |  | X | X |  |  |
ACD supervisor-tel. |  |  |  |  |  | X |  |  |  | X | X |  |  |
Alarm function |  |  |  |  | * | * | * |  |  | * | * | * |  |
Authority code |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Automatic callback | X | X | X | X | X | X |  | X | X | X | X |  | X | X
Automatic Redial |  |  |  | X | X | X | X | X | X | X | X |  |  |
Automated Attendant |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Background Music |  |  |  | X | X | X | X |  |  | X | X |  |  |
Bypass call diversion and follow me |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Call metering |  |  |  |  |  | * | * |  |  | * | X | * |  |
Call p. up-common |  |  |  |  | X | X | X |  |  | X | X | X |  |
Call p. up- ext. group | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Call p. up- individual | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Call waiting indic. | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Camp on | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Clock and diary |  |  |  |  |  | X | X |  |  | X | X | X |  |
Common bell | X | X | X | X | X | X | + | X | X | X | X | + | X | X
Conference | X | X |  | X | X | X | * | X | X | X | X | * | X | X
Conn. state mess. | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Conversation record. |  |  |  | X | X | X |  |  | X | X | X |  |  |
CT (Computer Telephony) | * | X | X | X | X | X |  | X | X | X | X |  | X | X
CTI-Groups |  | X | X | X | X | X | X | X | X | X | X | X | X | X
DISA |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Dictaphone function |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Diversion direct | ^ | X | X | X | X | X | # | X | X | X | X | # | X | X
Diversion on busy | X | X | X | X | X | X |  | X | X | X | X |  | X | X
Div. on no reply | X | X | X | X | X | X | # | X | X | X | X | # | X | X
Doorph. (answering) | X | X | * | X | X | X | X | X | X | X | X | X | X | X
Fault indication |  |  |  |  |  |  | X |  |  |  | X | X |  |
Follow me | ^ | X | X | X | X | X |  | X | X | X | X |  | X | X
Group hunting | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Hot line | X | X | X | X | X | X |  | X | X | X | X |  | X | X
Hotel guest room tel. | X | X | X | X |  |  |  | X | X |  |  |  | X | X
Hotel reception tel. |  |  |  |  |  | X | X |  |  |  | X | X |  |
Hotel service tel. |  |  |  |  |  | X |  |  |  | X | X |  |  |
Immediate answer |  |  |  |  | X | X |  |  |  |  | X |  |  |
Information | ^ | X | X | X | X | X | X | X | X | X | X | X | X | X
Inquiry | X | X |  | X | X | X | X | X | X | X | X | X | X | X
Intercom |  |  |  |  | X | X | * |  |  | X | X | * |  |
Intrusion | X | X | X | X | X | X | X | X | X | X | X | X | X | X
ISDN Caller List |  |  |  |  |  | X |  |  |  |  | X |  |  |
ISDN Calling Line Id. |  |  |  |  |  | X | X |  |  |  | X | X | X | X
ISDN Connected Line Identification |  |  |  |  |  | X | X |  |  |  | X | X | X | X
Key system function |  |  |  |  | X | X | X |  |  | X | X | X |  |
Last ext.numb.redial | ^ | X | X | X | X | X | X | X | X | X | X | X | X | X
Least Cost Routing | X | X | X | X | X | X | X | X | X | X | X | X | X | X
Loudspeaker paging |  |  |  | * | X | X | * |  |  | X | X | * |  |
Mailbox-sys. comm. |  |  |  | * | X | X | X | * | * | X | X | X |  |
Mailbox-sys. indiv. |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Message-sys. voice |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Message-s. call me |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Message-sys. text |  |  |  |  |  | X | X |  |  |  | X | X |  |
Name selection |  |  |  |  | X | X | X |  |  | X | X | X |  |
Night service | ^ | * | * | * | X | X | X | * | * | X | X | X | * | *
Paging | ^ | X | X | X | X | X | X | X | X | X | X | X | X | X
Park.for com.access |  |  |  |  | X | X | X |  |  | X | X | X | X | X
Parking individual | X | X |  | X | X | X | X | X | X | X | X | X | X | X
Private trunk line |  |  |  |  | X | X | X |  |  | X | X | X |  |
Programmable and fixed keys |  |  |  |  | 10 | 30 | 20 |  |  | 10 | 30 | 20 |  |
Refer back | X | X |  | X | X | X | X | X | X | X | X | X | X | X
Reminder service |  | X | X | X | X | X | X | X | X | X | X | X | X | X
Saved ext. nr. redial |  | * | * | X | X | X | X |  | X | X | X | X |  |
Secretary function |  |  |  |  | X | X |  |  |  |  | X |  |  |
Supervision |  |  |  |  | X | X | X |  |  | X | X | X |  |
Tandem - Slave | X | X | X | X | X | X |  | X | X | X | X |  | X | X
Tandem - Master | * | * | * | * | X | X |  | * | * | X | X |  | * | *
Telephone directory |  |  |  |  |  | X | X |  |  |  | X | X | * | *
Trunk line key |  |  |  |  | X | X | X |  |  | X | X | X |  |
Voice mail box, ext. |  | X | X | X | X | X | X | X | X | X | X | X | X | X

* |  | available with limitations

^ |  | available if you use the feature: "Abbreviated number dialling - common numbers"

+ |  | can not be programmed as Common bell, but only answer calls

# |  | corresponds to the feature "Offduty position"

Revision: PC1 © Ericsson Enterprise 2003