BusinessPhone Communication Platform 5.1
Commands > Commands 8000...8999

## 8501
Individual message welcome 1

In this command the reference number for the first part of the welcome message (when a call is diverted to the individual mailbox system) is stated.

Each welcome announcement consists of two parts. The first part is always played when a call is diverted to the individual mailbox system. If the directory number of the extension is to be played (see command 8502 Announce directory number?), the second part of the welcome announcement (see command 8503 Individual message welcome 2) is also played. This welcome message is used when an extension is diverted to the individual mailbox system. It is possible to record one welcome message per tenant group.

The given reference is supposed to have been recorded according to command 4415 Welcome individual. Note that recording according to command 4415 is only possible on a VMU-HD board.

Valid values: 0-31

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003