BusinessPhone Communication Platform 5.1
Warning Messages ASB 150 02 >

## 0xBB
E2DATA Conversion Overflow

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | CE |
Category: |  | MAINTENANCE |

The warning is used, when there was insufficient E2-memory to convert namestrings in the telephone directory.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

Revision: PH2 © Ericsson Enterprise 2003