BusinessPhone Communication Platform 5.1
Dialogs

## EURO Introduction

You can define the country specific settings for the EURO. To access the dialog, select the BP system in the Configuration tree view, press the left mouse button to open the context menu and select “EURO”.

Note

The “EURO” option is only available in online mode. Additionally, you must have the respective access rights to use the feature.

#### Dialog Description

Country | Select a country.
Currency | Currency abbreviation
System | Name of the BusinessPhone system
Round-up | Select the number of the digits that should appear after the coma
Enable operator | Enter the directory number of the operator. This way, you can also use the button to enable or disable outgoing calls.
Operator | Directory number of the operator.

#### Actions

Submit |  | To write the data displayed in the “New values column” to the BP system. |
Cancel |  | To cancel the conversion and to return to the Software/Firmware Upgrade: System selection dialog. |
Convert |  | To convert the values displayed in the “Old values”/ “Current” column. After converting, they will appear in the “New values” column. |
Reset |  | This button is available after submitting the converted data. Click on Reset to restore the original data from the log file and to display the data in the “Old values” column. The name of the column changes to “Original values”, indicating that these are the values before the conversion was performed. |
View logs |  | To show the log entries in text format. Log entries are generated for each converted system. The entries are saved in the log file on the computer running BMS server. However, it is possible to load, print, and view these files using the “View Log files” button. Please note that each file is named by the system ID. If no characters are allowed (e.g. system identifier), they will be replaced with proprietary strings. |
Disable outgoing calls |  | To reroute all outgoing calls to the operator. |
Enable outgoing calls |  | To enable outgoing calls for all extensions (according to the configuration). |
Block trunks |  | To block outgoing calls. |
De-block trunks |  | To suspend the blocking of outgoing calls. |
Enable CM |  | To enable the Call Metering feature. |
Disable CM |  | To disable the Call Metering feature |

Revision: B © Ericsson Enterprise 2003