BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4901
Number of participants

This command is used to state the maximum number of conferees (participants) permitted in a conference. The number includes external lines (conferees).

Range of values = 3-6

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003