BusinessPhone Communication Platform 5.1
Commands > Commands 4000...4999

## 4004
Cyclical selection

This command is used to state the search principle to be used for the selection of operators.

Y = Sequential search basis - the operator who has been free longest shall be selected |  |

N = Sequential selection - search for a free operator always starts at the first operator in the group. If the first operator is busy, the second will be chosen, and so on. |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: PD1 © Ericsson Enterprise 2003