BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 7F REALTIME

00h RTCMIN01 |  | Every minute |
01h RTCMIN05 |  | Every 5:th minute |
02h RTCMIN15 |  | Every 15:th minute |
03h RTCMIN30 |  | Every 30:th minute |
04h RTCMIN60 |  | Every 60:th minute |
04h RTCHOUR01 |  | Every hour (same as 60 min) |
05h RTCHOUR03 |  | Every 3:rd hour |
06h RTCHOUR06 |  | Every 6:th hour |
07h RTCHOUR12 |  | Every 12:th hour |
08h RTCHOUR24 |  | Every 24:th hour |
40h RTCWR |  | Write time in time circuit |
41h RTCWRANSW |  | Answer after a write |
50h RTCRD |  | Request real time |
51h RTCRDANSW |  | Answer after a read |
60h RTCMINUTE |  | Periodical minute-message from RP |

Revision: F © Ericsson Enterprise 2004