BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x4F
RP Illegal Hardware State

Default definition: |  | ERROR |
Used by block: |  | BTU, CPU-D4, ELU-A |
Category: |  | DESIGNER |

The hardware state is checked, when a trunk or extension line is idle. This warning is sent, when an illegal state is detected. The illegal state is corrected.

- D1: Individual number
- D2: Illegal state
- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004