BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5501
Delete a route

In ASB 150 a route is a list of trunk lines. When the route’s directory number is called a free trunk is seized in accordance with a defined allocation principle.

This command will delete a route with the stated directory number.

There is one specific route in the system (which INITIALLY has directory number 0 - but can have been altered to another) which MUST NOT be deleted. The directory number of this route will NOT be displayed in the list - if it is the only route in the system, the list will not be displayed at all.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004