BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5406
Create call pickup ext. group

In ASB 150 a call pickup group is formed from a list of extensions. In case of a call to a member of the group another member can answer the call from his/her own telephone by dialling the digit for “group call pickup”.

A new group for group call pickup can be created via this command.

ASB 150 permits a maximum of 16 of these groups.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004