BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5207
Login fail bar time

This command indicates the number of minutes during which the PABX will be barred for login, if too many unsuccessful log-in attempts are detected. Value 0-255 minutes.

This time applies only if command 5206 Login fail action has been entered to bar the PABX after too many consecutive invalid passwords have been received.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004