BusinessPhone Communication Platform 6.0
Dialogs

## Task Scheduler

Enables automatic configuration & maintenance.

To access the dialog, click on the “Task Scheduler” menu in the Tools directory tree.

Scheduled tasking allows executing multiple configuration tasks, at specific time(s) in particular BusinessPhone systems the BMS server is allowed to connect to.

It is possible to select any BMS session to be executed at the users preferred time. Additionally, specific functions like changing the system password, setting the system time or executing a system backup can be initiated from one single BMS server.

##### 5 Task types can be selected from:

- Change Password
- Run Script
- Create Backup
- Set Time
- Download Firmware to D4 Equipment

#### Procedure:

1. Select the PBX-system(s), on which the selected Task type should be run.

1. Via the System List, select the PBX-system(s) and press the “Close”-Button.

2. The “Task description” is your individual task name.
3. State in the “Start Date (yyyy/mm/dd)” and “Start Time” fields when the task should be executed the first time.
4. The “Time Offset” is only valid for the task “Set Time”. Enter the time difference caused of different time zones the PC and the to be synchronized PBX are located in.
5. Enter how often the Task should be repeated in the “Type of scheduling” field.
6. Press “Submit” to include the new task in the Task Scheduler Status list.

Note

By default a new task is NOT in active status!

#### Actions

View Logs |  | To activate the selected task |
Activate |  | To activate the selected task |
Deactivate |  | To deactivate, but not delete the selected task |
Delete |  | To Delete the selected task |
Refresh |  | To refresh the dialog. |
New Task |  | To select a new task |

Revision: B © Ericsson Enterprise 2004