BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4314
Simult retrievings

This command is used to restrict the number of callers simultaneously retrieving messages from the message system. This is of particular importance when messages are retrieved from extensions without display or from external parties. In these cases voice prompts are used to guide a caller through a session. To play voice prompts, a voice channel on the VMU-board is required. In order to avoid that a message sending session is blocked because several retrieving sessions use the voice prompt, the number of simultaneous retrieving sessions is restricted.

##### Valid data

1..16 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004