BusinessPhone Communication Platform 6.0
System Overview ASB 150 02 Release 14 (BusinessPhone 6.0) > Telephone Types > Analog Telephones

## Dialog 4186 High, DBC 186

- 2x24 characters display, possible to tilt
- Alarm function
- Built-in phone book (50 entries)
- Program key (can be deactived - by a switch at the bottom)
- Delete, Pause and Redial key
- Message waiting lamp
- 10 dial-by-name keys
- Loudspeaker
- Group listening
- Hands-free speaker
- Flash time for R-key programmable
- DTMF signalling
- Tone ringer
- For display, clock and programming an external power feeding (9 VAC) is needed.
- The Dialog 4186 has an E2 memory.
- a/b Dataport for the connection of Laptop-modems, faxes etc.
- Wall mounting possible

Revision: B © Ericsson Enterprise 2004