BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3301
Random Selection

This command defines the selection principle to be used for a route.

Yes = |  | sequential selection with alternating start point. Search for a free trunk starts with the position number following that of the latest seized trunk.

No = |  | sequential selection from first trunk. Search for a free trunk always starts at the first trunk in the route.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004