BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2057
Follow me/Diversion to ACD

The command defines whether follow me, direct diversion or diversion on busy to an active ACD group is allowed-on default the command is deactivated, that means follow me, direct diversion respective diversion on busy is not allowed.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004