BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5205
Login fail limit

This command defines a limit for the number of consecutive invalid passwords that may be entered before corrective action is taken.

##### Valid data

0-99 |

If the limit is exceeded, the action chosen in command 5206 Login fail action will be taken.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004