BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1962
Predigits to be removed for calling/connected number if TON=National

This command is used to define the number of predigits to be removed from a received CLI/COL with type of number NATIONAL (E.164).
It is used to remove a prefix before a CLI/COL is displayed or sent forward to the private network.

This command is valid for both T/Q interfaces.

##### Valid data

00-15 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004