BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1502
Tariff number

This command is used to define, for the selected trunk line, which tariff model (0-5) is used for call cost calculation.

Six different tariff (models) per carrier (network operator) can be used for cost metering (see command 8430 Customer tariff (cost per pulse) 0 - 8435 Customer tariff (cost per pulse) 5.

If the tariff model should not be used, then this command must be set to the default value and cost calculation is done with cost per pulse stored via command 8424 Multiplication factors.

Value = 0-5

default: blank (not programmed)

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004