BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2263
Type of individual number translation

This command defines the search algorithm in the 2260 DDI/CN number translation, for internal calls.

The command value refers to the system defined individual number translation tables “DDI1 and/or DDI2”. The contents of these tables is used for the translation of directory number from DDI format to internal format and vice versa.

“Type of individual number translation” has to be in harmony with the current setting for command 1804 DDI number translation, as both commands use the same “Individual number translation table”.

The following command values are accepted:

Value | Description
0 | DDI number translation for internal calls is disabled (DEFAULT)
1 | DDI number translation according to table “DDI1”
2 | DDI number translation according to table “DDI2”
3 | DDI number translation according to tables in order “DDI1” and “DDI2”
4 | DDI number translation according to tables in order “DDI2” and “DDI1”

If DDI number handling for internal calls is enabled, then the user will dial and see DDI numbers instead of internal directory numbers. Disabling the DDI number handling for internal calls the user interface remains unchanged.

Note

The DDI number translation for internal calls makes possible to configure a homogenous number plan with unique directory numbers up to 8 digits within the whole corporate network.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004