BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4304
Time to keep message

This command states for how many full days (24-hour periods) a message is to be stored (1-99). Counting starts at middnight after the message has been sent. Erasure of messages takes place at midnight following the programmed number of 24-hour periods. The longer the message is stored the greater is the risk that the message memory will reach its full capacity.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004