BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0187
Expensive Route Warning Tone

This command defines, if the user shall be informed about an alternatively choosen PNR route (e.g. especially if it as public route) for the ongoing call setup.

For generating the Expensive route warning tone, the corresponding commands for the route must also be programmed (see command 9128 Send expensive route warning tone 2, 9138 Send expensive route warning tone 3, 9148 Send expensive route warning tone 4).

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004