BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 5C MUCTRL

00h MUIDLECHN |  | Background music PCM channel |
01h MUHOLDCHN |  | Music on hold PCM channel |
02h MUACK |  | Answer msg for subcodes MUIDLECHN and MUHOLDCHN |
03h MUNAK |  | Answer msg for subcodes MUIDLECHN and MUHOLDCHN |
04h MUANNOLOADED |  | Inform that announcements are loaded |

Revision: F © Ericsson Enterprise 2004