BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4322
Maximum number of OCN trunks

This command determines how many trunks are allowed to be used simoultanously for outcall notification calls.

In 4320 Notification scheduling profile - the maximum number of used trunks in dependence of

- max. amount of users and
- min. scheduling profile,

are described.

To prevent a wrong configuration of the system, the following trunks, which are described in the table, have to be used in dependance of max. amount of users.

Revision: E © Ericsson Enterprise 2004