BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0301
Key function

This menu shows the function of the progammable keys for the selected extension.

This command states which function a key is to have.

For some key functions it is possible to program an associated number, how incoming calls are to be presented and ACD-group priority. See also commands 0302 Number/ID, 0303 Ringing alternative and 0304 ACD-group priority.

On initiation of the system, all programmable keys are assigned the function "name selection" (see below).

If a different function is required the key will have to be redefined.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

##### Valid data

Name Selection (Default) |  | 10 |
Suffix Dialling |  | 11 |
External Line |  | 12 |
Supervision |  | 13 |
Intercom |  | 14 |
Voice Paging |  | 15 |
ACD Group |  | 16 |
ACD Supervision |  | 17 |
Common Mailbox-supervision |  | 18 |
Slave Supervision |  | 19 |
R-key |  | 25 |
Busy Line 2 / Free 2nd Access |  | 26 |
Conference |  | 27 |
Immediate Answer |  | 28 |
ACD Ready |  | 29 |
Account Code |  | 30 |
ACD Clerical |  | 31 |
ACD Help |  | 32 |
Operator - Hold |  | 33 |
External Voice Mailbox |  | 34 |
Common Hold |  | 35 |
Transfer |  | 36 |
Save/Redial |  | 37 |
Read& |  | 38 |
Enter |  | 39 |
Number Secrecy |  | 40 |
MCID key |  | 41 |
Logon/off Slave |  | 43 |
ACD Pause |  | 44 |
Conv. Recording |  | 45 |

Revision: F © Ericsson Enterprise 2004