BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2044
Attenuation factor for loudspeaker paging group 4

This command indirectly defines the volume that will be used with loudspeaker paging for a specific loudspeaker paging group. This volume, however, is a relative volume with an attenuation factor rather than a real volume.

In loudspeaker paging operation, the volume is sent to all extensions. If there is no individual volume programmed, the extensions employing loudspeaker paging use this common volume. If an individual volume is programmed, this volume will be used instead.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004