BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0165
Diversion on no reply to slave?

The command defines whether or not a diversion on no reply to an associated logged off slave extension should be done. If the extension is a master and a member of a tandem configuration the command data shall be copied to the slave and blocked for the slave’s further use.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004