BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8502
Announce directory number?

When an extension has activated diversion to the individual mailbox system, all incoming calls are diverted to the message storing facility.

An external caller or an internal party without display and function keys will be guided through the session with voice prompts.

The first voice prompt is a welcome message explaining that the called extension has activated diversion to the mailbox system. If the directory number is to be included (yes), voice prompt welcome 1, storing + directory number + welcome 2, storing is played (see commands 8501 Individual message welcome 1 and 8503 Individual message welcome 2 for the voice prompts).

If the directory number is not to be included (no), only welcome 1, storing is played.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004