BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xD7
CIL Memory Capacity Exceeded

Default definition: |  | ALARM + INFO + EXTERN + ACTIVE |
Used by block: |  | CL |
Category: |  | MAINTENANCE |

500 CIL/HOTEL records are stored. The maximum storage capacity has been exceeded.

- D1:
- D2:
- D3: Undefined
- D4: Undefined

#### Recommended action

Verify the programming of the external (peripheral) equipment and the programming of the IO-channels.

Revision: I © Ericsson Enterprise 2004