BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8732
Error announcement reference

When an external or internal party connected to a CTI Group (see command 5428 Create CTI Group) sends a customer-id which is longer than 16 digits, the playing of an error announcement will be started to inform the caller about the faulty request. This announcement will also be played in case of a wrong directory number selection or missing resources (VMU). In this command the voice reference for the announcement is stated.

The given reference is supposed to have been recorded according to command 4426 CTI-AA prompts 1-24. Note that a recording in command 4426 is only possible on a VMU-HD board.

##### Valid data

1-24 |  |  |
(blank) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004