BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3030
Day/night trunk group 8

This command is used to state for which A-categories it is permitted to alter the function for day/night switching for trunk group 8. The procedure for day/night switching =*88#.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004