BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8455
Pulse rate table general (list price)

This command is used if the calculation of a fictive call is based on pulse rates. Up to 44 pulse rate tables (0-43) with 16 different relative cost levels (0-15) can be specified. Each relative cost level consists of initial pulse and pulse frequency. Both factors are used to calculate the cost of a fictive call.

Pulse rate table: |  | 0-43 |
Initial pulse: |  | 0-255 |
Pulse frequency: |  | up to 10 digits incl. decimal point |
Unit: |  | Hz (based on pulses per second) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004