BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0151
Tenant group

The command defines which tenant group the extension belongs to in a multi PABX application.

In detail this means that if several customers share one ASB 150 they can separate their extensions into a maximum of 16 tenants.

##### Valid data

Master only |  | copied to slave (0-15) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004