BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5626
Alter individual mailbox directory number

This directory number is used for the message facility. An extension can set diversion or follow-me to this directory number. In that case all calls to the extension are diverted to the individual mailbox system where the caller can leave a voice message to the extension. If the directory number is called directly, messages for an extension can be retrieved.

Note

Command 5426 Create individual mailbox is used to create directory number for this facility.
Command 5526 Delete individual mailbox number is used to delete directory number for this facility.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004