BusinessPhone Communication Platform 6.0
Dialogs

## IP-Extension Administration Table

This dialog shows detailed information about the IP extensions in your system:

- # GW

- Number of the gateway

- IP address

- A unique, 32-bit number for a specific TCP/IP host on the Internet. Usually printed in decimal form (for example, 128.122.40.227).

- Status

- The current status of the IP extension:
- - .... Value not set
- C.... Confirmed
- R.... Registered

- Terminal

- The terminal of the IP extension.

- Client IP

- The IP address of the client.

- Q.931 port

- ITU-T standard. Describes call signalling.

- RAS port

- ITU-T standard. Describes call signalling.

- DirNo and ID

- The extension’s directory number and its ID.

#### Actions

Back |  | To return to the Gatekeeper Data dialog. |
Reload |  | To retrieve the current system settings. |

Revision: B © Ericsson Enterprise 2004