BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3036
Program loudspeaker paging key

In order to be able to restrict the number of extensions with access to certain facilities, such extensions are assigned A-category (ACOS) via command 0101 Facility COS.

The extensions can have a number of programmable keys with different functions. See command 03.

If an extension wishes to alter the function of a key, the user must be authorised to program keys for both the old and the new functions.

This command is used to state for which A-categories it is permitted to program a key for loudspeaker paging.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004