BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1030
Public number group

The command is used to assign a trunk to a group of trunks which have all one and the same public number (e.g a PRA) . The assignment to the group defines which of the 32 public numbers (command 2220 Public number) should be used to create the A/B-number to be sent to the network on request.

##### Valid data

0 |  | (default) |
1-31 |  |  |

Default data: group 0

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004