BusinessPhone Communication Platform 6.0
Dialogs

## Radio Exchange

This dialog gives you an overview about the hardware of your DECT system. The list shows all boards and board parts of the system.

This dialog is also used to reset a board and to replace or remove a board if on ICLU.

#### Dialog description

Address |  | The address of the board. |
Board type |  | The type of board, e.g. CPU, CLU, SPU or DTU. |
SW version |  | The software version that is used on-board. |
Status |  | Shows if the board is available within the system. |
Properties |  | For further information about a board, click on this link. Depending on the type of board, the ABC number (CPU), the status of the base station (CLU), the circuit (SPU), or of layer 1 or layer 2 will be shown. |

#### Actions:

Reset |  | To reset a certain part of the ICCU. Board type CPU: System reset Board type CLU, SPU: Reset, remove/replace if on ICLU Board type DTU: Reset |
Replace |  | To replace a board of the system with another board. Necessary for ICLU-boards. |
Remove |  | To remove a board from the system. Necessary for ICLU-boards. |

Revision: B © Ericsson Enterprise 2004