BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8797
CTI Groups

This command group consists of commands to define the parameters for the facility CTI Groups. First one or more directory numbers for the facility CTI Groups (see command 5428 Create CTI Group) must be created. By entering this command group, an existing directory number must be entered. Now all parameters are related to this voice menu.

Command 8730: |  | Defines the general announcement for CTI Groups. A special announcement group exists for this facility (see command 4426 CTI-AA prompts 1-24) which is designed to contain voice prompts for 16 voice menus. |
Command 8731: |  | Defines the instruction announcement for the menu (see command 4426 CTI-AA prompts 1-24). |
Command 8732: |  | Defines the error announcement for the menu (see also command 4426 CTI-AA prompts 1-24). |
Command 8733: |  | Defines the default exit position in case of response or resource errors. |

Revision: D © Ericsson Enterprise 2004