BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3086
Day/night ACD group 3

This command is used to state which A-categories are permitted to alter the function of day/night switching with respect to ACD group 3.

The procedure for day switching = |  | *893 |
The procedure for night switching = |  | *893 (toggle function) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004