BusinessPhone Communication Platform 6.0
VMU-HD & MFU

## Title 21: Mailbox Content Information (Command 4433 (lang1) - 4434 (lang 2) - 4435 (lang 3))

No | Filename language 1 | Predefined texts | Filename language 2 | Filename language 3
0 | D4D0D4D0.001 | You have ... | D4FOD4FO.001 | D51OD51O.001
1 | D4D1D4D1.001 | ... and ... | D4F1D4F1.001 | D511D511.001
2 | D4D2D4D2.001 | You have no messages. | D4F2D4F2.001 | D512D512.001
3 | D4D3D4D3.001 | ... new message | D4F3D4F3.001 | D513D513.001
4 | D4D4D4D4.001 | ... new messages | D4F4D4F4.001 | D514D514.001
5 | D4D5D4D5.001 | ... heard message | D4F5D4F5.001 | D515D515.001
6 | D4D6D4D6.001 | ... heard messages | D4F6D4F6.001 | D516D516.001
7 | D4D7D4D7.001 | ... stored message | D4F7D4F7.001 | D517D517.001
8 | D4D8D4D8.001 | ... stored messages | D4F8D4F8.001 | D518D518.001
9 | D4D9D4D9.001 | ... one ... (Note: article for 1 message) | D4F9D4F9.001 | D519D519.001
10 | D4DAD4DA.001 | Thank you for calling. Good-Bye. | D4FAD4FA.001 | D51AD51A.001
11 | D4DBD4DB.001 | No new messages. | D4FBD4FB.001 | D51BD51B.001
12 | D4DCD4DC.001 | No heard messages. | D4FCD4FC.001 | D51CD51C.001
13 | D4DDD4DD.001 | No stored messages. | D4FDD4FD.001 | D51DD51D.001
14 | D4DED4DE.001 | There is no previous message. | D4FED4FE.001 | D51ED51E.001
15 | D4DFD4DF.001 | Message retrieval:- To listen to new messages,press ONE, To listen to messages already heard, press TWO. | D4FFD4FF.001 | D51FD51F.001
16 | D4E0D4E0.001 | To replay, press ONE, For time stamp, press THREE, For the previous message, press SEVEN, For the next message, press NINE, To delete it, press HASH, To delete it and call the extension, press STAR. | D500D500.001 | D520D520.001
17 | D4E1D4E1.001 | To replay, press ONE, For time stamp, press THREE, To pause or continue during replay, press FIVE, For the previous message, press SEVEN, For the next message, press NINE, To delete this message, press HASH. | D501D501.001 | D521D521.001
18 | D4E2D4E2.001 | End of messages:- For the last message, press SEVEN, To return to message retrieval, press NINE, To exit, hang up. | D502D502.001 | D522D522.001
19 | D4E3D4E3.001 | Forwarded message from mailbox ... (+ number of MBX sender) | D503D503.001 | D523D523.001

e.g.: “You have no messages”
e.g.: “You have” - “one” - “new message”(one = 4433 - 9)
e.g.: “You have” - “two” - “new messages” (two = 4405 - 1)
e.g.: “You have” - “one” - “heard message”
e.g.: “You have” - “two” - “heard messages”
e.g.: “You have” - “one” - “stored message”
e.g.: “You have” - “two” - “stored messages”
e.g.: “You have” - “one” - “new message” - “and” - “one” - “heard message”
e.g.: “You have” - “one” - “new message” - “and” - “one” - “stored message”
e.g.: “You have” - “one” - “heard message” - “and” - “one” - “stored message”
e.g.: “You have” - “one” - “new message” - “one” - “heard message” - “and” - “one” - “stored message”

Revision: E © Ericsson Enterprise 2004