BusinessPhone Communication Platform 6.0
Dialogs

## Service Logbook

The feature Service Logbook is only available in full access mode and located in the menu maintenance.

If there is no Service Logbook in the ASB 150 02 system the user has to possibility to choose a peripheral board for further Service Logbook usage.

When a Service Logbook is detected on any peripheral board in the ASB 150 02 system file display is offered. In case of an existing Logbook there is no possibility to create an additional Service Logbook by the means of another board. If there is any board in shutdown mode, no new Service Logbook can be created. If there are more than one Service Logbook in the system detected the user can choose one of them for deletion.

New entries in the Service Logbook will be added in the following way. The user has to enter the date (english format of date), User name (maximum 25 characters) and any additional text (maximum 500 bytes).

All data are stored in plain text format with the line termination CR/LF.

2002.08.20 WHOIAM1CR/LF
_Entry_number1CR/LF
2002.08.25 WHOIAM2CR/LF
_This_is_a_long_entry_number2CR/LF
_This_is_another_long_entry_number3CR/LF

Note

_ stands for SPACE

If the maximum file size exceeds 3 kBytes, the oldest entry has to be deleted.(FIF0).

The Service Logbook can be dumped with System Logs in Dumpfiles - File Manager.

Revision: B © Ericsson Enterprise 2004